**Glass and Dishwasher PROFI with deeper wash chamber**

**Model: Profi FXL-10B**

|  |  |
| --- | --- |
| Type | One Tank Glass and Dishwasher with extra deep wash chamber 640 mm |
| Rack Size | 500 x 500 mm  500 x 530 mm  600 x 400 mm (EN-boxes, trays) |
| Design | Front door machine, adjustable as undercounter model |
| Capacity | 40 Racks/h / 720 Plates/h / 1440 Glasses/h |
| Voltage | 400/50/3 (230/50/1) |
| Tank, Frame and Panels | Stainless steel 18/9 |
| Wash result | According to DIN10512 section 7 |

|  |  |
| --- | --- |
| Ready to install: | |
| - fill and drain hoses  - power cord (400 V-connection)  - detergent dispenser  - rinse agent dispenser  - rinse pump  - drain pump  - non-return valve | |
| Wash pump with smart start  Automatic Tank Fill  Multi-Phasing | |
| **Rack equipment** | |
| 1 Plate Rack P-18-12  1 Insert for sheets 324660  1 Cutlery Rack with 4 boxes 01-246175-1 | |
| **Product Advantages**  • **XL wash chamber:**  suitable to wash trays of 600 x 400 mm. Ideal for fast-food restaurants, cafés and snack bars  • **VISIOTRONIC-TOUCH control:**  colour touchscreen (displays text and graphic) in conjunction with single-button control and remaining cycle time indication.  • **WASHSMART APP:**  Controlling your warewash operation with smart technology: status and messages, usage and operating costs, hygiene, service and consumables order  • **SENSO-ACTIVE resource management:**  constantly measuresthe quality of the wash water andkeeps the amount of rinsing neededin each rinse cycle to the minimumin order to guarantee a fully hygienicwash result  • **2IN1 double rack system:**  two racks can be washed in a single wash cycle. One rack of cups can be washed underneath, while a second rack containing dishes and cutlery can also be washed above it. Thanks to the optimum use of the entire wash chamber the performance of the machine can be doubled  • **CLIP-IN wash and rinse arms**:  wash and rinse arms can be removed with one hand and without any tools  • **Intelligent data documentation:**  automatic recording of important operational data and consumptions and indication on the display  • **USB-interface:**  Comfortable download of operational data in form of a protocol via USB  • **GENIUS-X² fine filter system:**  advanced filter system with prewash function reduces detergent consumption up to 35%  • **Interlocked strainer**:  prevents operation without tank strainer  • **Optional refill signal:**  Monitors contents of external as well as integrated chemical containers  • **Hygiene programme:**  for removal of calcium carbonate and other deposits from the wash chamber | |
| **Technical Data:** | | |
| Machine housing width | 600 mm |
| Machine housing Depth | 640 mm |
| Depth when Door is open | 1088 mm |
| Height | 825 mm |
| Loading height | 425 mm |
|  | |
| Cycle time\*\* | 90 / 180 / 360 sec.  and special programs |
| Capacity\*\* | Up to 40 Racks/h / 720 Plates/h / 1440 Glasses/h |
| Wash temperature | 63 °C |
| Rinse temperature | 82 °C |
| Tank capacity | 10,6 l |
| Fresh water consumption/Rack | 2 l |
|  | |
| Booster loading | 6,2 kW (2,1 kW) |
| Total loading | 6,8 kW (2,7 kW) |
| Pump power | 0,5 kW / 350 l/min |
| - | 3x16 A (16 A) |
| Voltage | 400/50/3 (230/50/1) |
|  | |
| \* To reach set rinse temperatures even with cold water connection, the actual cycle-times extend accordingly. | |
| \*\* Theoretical performance | |

