**Glass and Dishwasher PROFI with deeper wash chamber**

**Model: Profi FXL-10B**

|  |  |
| --- | --- |
| Type | One Tank Glass and Dishwasher with extra deep wash chamber 640 mm |
| Rack Size | 500 x 500 mm500 x 530 mm600 x 400 mm (EN-boxes, trays) |
| Design | Front door machine, adjustable as undercounter model  |
| Capacity | 40 Racks/h / 720 Plates/h / 1440 Glasses/h  |
| Voltage | 400/50/3 (230/50/1)  |
| Tank, Frame and Panels | Stainless steel 18/9  |
| Wash result | According to DIN10512 section 7  |

|  |
| --- |
| Ready to install: |
| - fill and drain hoses- power cord (400 V-connection)- detergent dispenser- rinse agent dispenser- rinse pump- drain pump- non-return valve  |
| Wash pump with smart start Automatic Tank FillMulti-Phasing |
| **Rack equipment** |
| 1 Plate Rack P-18-121 Insert for sheets 3246601 Cutlery Rack with 4 boxes 01-246175-1 |
| **Product Advantages** • **XL wash chamber:** suitable to wash trays of 600 x 400 mm. Ideal for fast-food restaurants, cafés and snack bars• **VISIOTRONIC-TOUCH control:**colour touchscreen (displays text and graphic) in conjunction with single-button control and remaining cycle time indication.• **WASHSMART APP:** Controlling your warewash operation with smart technology: status and messages, usage and operating costs, hygiene, service and consumables order• **SENSO-ACTIVE resource management:** constantly measuresthe quality of the wash water andkeeps the amount of rinsing neededin each rinse cycle to the minimumin order to guarantee a fully hygienicwash result• **2IN1 double rack system:** two racks can be washed in a single wash cycle. One rack of cups can be washed underneath, while a second rack containing dishes and cutlery can also be washed above it. Thanks to the optimum use of the entire wash chamber the performance of the machine can be doubled• **CLIP-IN wash and rinse arms**: wash and rinse arms can be removed with one hand and without any tools• **Intelligent data documentation:**automatic recording of important operational data and consumptions and indication on the display• **USB-interface:** Comfortable download of operational data in form of a protocol via USB• **GENIUS-X² fine filter system:**advanced filter system with prewash function reduces detergent consumption up to 35%• **Interlocked strainer**: prevents operation without tank strainer• **Optional refill signal:** Monitors contents of external as well as integrated chemical containers• **Hygiene programme:** for removal of calcium carbonate and other deposits from the wash chamber |
| **Technical Data:**  |
| Machine housing width | 600 mm |
| Machine housing Depth | 640 mm |
| Depth when Door is open | 1088 mm |
| Height | 825 mm |
| Loading height | 425 mm |
|   |
| Cycle time\*\* | 90 / 180 / 360 sec. and special programs |
| Capacity\*\* | Up to 40 Racks/h / 720 Plates/h / 1440 Glasses/h |
| Wash temperature | 63 °C |
| Rinse temperature | 82 °C |
| Tank capacity | 10,6 l |
| Fresh water consumption/Rack | 2 l |
|   |
| Booster loading | 6,2 kW (2,1 kW) |
| Total loading | 6,8 kW (2,7 kW) |
| Pump power | 0,5 kW / 350 l/min |
| - | 3x16 A (16 A) |
| Voltage | 400/50/3 (230/50/1) |
|   |
| \* To reach set rinse temperatures even with cold water connection, the actual cycle-times extend accordingly.  |
| \*\* Theoretical performance  |

